**Title:** Designing Multiplexer (MUX) and Demultiplexer (DEMUX), Encoder and Decoder Circuits.

# Introduction:

In this experiment students will learn how to design and implement multiplexers (MUX) and demultiplexers (DeMUX) of different sizes using basic logic gates. They will also learn how to construct bigger multiplexer using smaller multiplexers. Students will also construct encoder and decoder circuits. Encoder and decoder circuits are very useful in information transmission, conversion, compression and maintaining the secrecy of any information.

# Theory and Methodology:

**Part I: Multiplexer and Demultiplexer**

A multiplexer (or mux) is a device that selects one of several inputs and forwards the selected input into a single line. A multiplexer of 2*n* inputs has *n* selection lines, which are used to select which input has to be sent to the output. A multiplexer is also called a data selector.

A demultiplexer (or demux) is a device taking a single input and selecting one of many data-output-lines, which is connected to the single input.

**Multiplexer:**

In computer system, it is often necessary to choose data from exactly one of a number of possible sources. Suppose that there are four sources of data, provided as input signals D0 ,D1, D2 and D3. The values of these signals change in time, perhaps at regular intervals. We want to design a circuit that produces an output that has the same value as either D0 or D1 or D2 or D3, dependent on the values of two selection pins S1 and S0. Here, the number of selection pin is two. Four combinations are possible using these two selection pins S1 and S0, such as (S1, S0) = (0,0), (0,1), (1,0), (1,1). Each combination is dedicated for each input. Let us consider the output variable is f. Now if S1 = 0 and S0 = 0 then f = D0, if S1 = 0 and S0 = 1 then f = D1, if S1 = 1 and S0 = 0 then f = D2 and if S1 = 1 and S0 = 1 then f = D3.

It is important to know that there is a relationship between the number of input and the number of selection pins. If the number of selection pin of a MUX is n, then maximum 2n inputs are possible for that MUX. And the MUX will be called as 2nto1 line MUX. The MUX we are going to design is a 4to1 MUX. There could be also 2to1 MUX, 8to1 MUX, 16to1 MUX etc.

For our design, there are 4 inputs and 2 selection pins. So actually we have 6 inputs. Now if we draw the truth table for 6 different inputs, there will be 64 input combinations. But fortunately we can do it in a more convenient way as given below.

## Table:1

|  |  |  |
| --- | --- | --- |
| S1 | S0 | f |
| 0 | 0 | D0 |
| 0 | 1 | D1 |
| 1 | 0 | D2 |
| 1 | 1 | D3 |

From the above truth table, we can write the function as given below.

𝑓= 𝑆1̅𝑆0̅𝐷0+𝑆1̅𝑆0𝐷1+𝑆1𝑆0̅𝐷2+𝑆1𝑆0𝐷3 … (1)

The logic circuit of the equation (1) is given in figure 1.

A diagram of a circuit

Description automatically generated

# Figure1: 4to1 Multiplexer

**Demultiplexer:**

A Demultiplexer or Demux is opposite to the multiplexer. It has only one input and several outputs and one or more selection pins. Depending on the combination of selection input, the data input will be routed to one of many outputs. Other inputs will be low. Depending on the number of output, demultiplexers are termed as 1to2, 1to4 and 1to8 demultiplexers etc. If the number of selection pin is n, then maximum 2n outputs can be accommodated.

We are going to design a 1to4 line demux having an input Din, two selection pins S1 and S0 and four outputs D0 ,D1, D2 and D3. Now if S1 = 0 and S0 = 0 then D0 = Din, if S1 = 0 and S0

= 1 then D1 =Din, if S1 = 1 and S0 = 0 then D2 = Din and if S1 = 1 and S0 = 1 then D3 = Din. We can draw the truth table as given below.

## Table:2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S1 | S0 | D0 | D1 | D2 | D3 |
| 0 | 0 | Din | 0 | 0 | 0 |
| 0 | 1 | 0 | Din | 0 | 0 |
| 1 | 0 | 0 | 0 | Din | 0 |
| 1 | 1 | 0 | 0 | 0 | Din |

From the above truth table we can write the functions for D0 ,D1, D2 and D3 as given below.

̅ … (3)

𝐷0=𝑆1̅𝑆0̅𝐷𝑖𝑛 … (2)

𝐷1=𝑆1̅𝑆0𝐷𝑖𝑛 … (3)

𝐷2=𝑆1𝑆0̅𝐷𝑖𝑛 … (4)

𝐷0=𝑆1̅𝑆0̅𝐷𝑖𝑛 … (5)

The circuit for 1to4 line demux is given below.

A diagram of a circuit

Description automatically generated

Figure 2: 1 to 4 Demultiplexer

It is also possible to construct 4to1 multiplexer (and 1to4 demultiplexer) using 2to1 multiplexers (1to2 demultiplexers) only. Figure 3 and figure 4 show the construction of 4to1 multiplexer using 2to1 multiplexers and 1to4 demultiplexer using 1to2 demultiplexers only.

A diagram of a diagram

Description automatically generated

Figure 3: 4to1 multiplexer using 2to1 multiplexers.

A black background with white lines

Description automatically generatedD0 D1

Din

D2 D3

S1 S0

Figure 4: 1to4 demultiplexer using 1to2 demultiplexers.

# Part II: Encoder and Decoder:


An encoder is a device or a circuit that converts information from one format or code to another. A decoder does the reverse operation of the encoder. It undoes the encoding so that the original information can be retrieved. Both the encoder and decoder are combinational circuits.

Encoding and decoding are very widely used ideas. They have applications in electronic circuits, software programs, medical devices, telecommunication and many others. In this experiment, a very basic 2-to-4 line decoder and a decimal to BCD encoder will be constructed.

A decoder can convert binary information from n input lines to a maximum of 2n unique output lines. The 2-to-4 line decoder will take inputs from two lines and convert them to 4 lines.

A B

D0



D1

D2

D3

**Fig.1:** 2-to-4 line decoder

The expressions for implementing 2-to-4 line decoder – D0 = A’B’

D1 = A’B

D2 = AB’ D3 = AB

Truth table for 2-to-4 line decoder is given below –

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| A | B | D0 | D1 | D2 | D3 |
| 0 | 0 | 1 | 0 | 0 | 0 |
| 0 | 1 | 0 | 1 | 0 | 0 |
| 1 | 0 | 0 | 0 | 1 | 0 |
| 1 | 1 | 0 | 0 | 0 | 1 |

A decimal to BCD encoder converts a decimal number into Binary Coded Decimal (BCD).

D0 D1 D2 D3 D4 D5 D6D7 D8 D9



Y0

Y1

Y2

Y3

**Fig.2:** Decimal to BCD encoder

The expressions for implementing the decimal to BCD encoder –

Y0 = D1 + D3 + D5 + D7 + D9

Y1 = D2 + D3 + D6 + D7 Y2 = D4 + D5 + D6 + D7 Y3 = D8 + D9

Truth table for decimal to BCD encoder is given below –

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Dec. | Y3 | Y2 | Y1 | Y0 |
| D0 | 0 | 0 | 0 | 0 |
| D1 | 0 | 0 | 0 | 1 |
| D2 | 0 | 0 | 1 | 0 |
| D3 | 0 | 0 | 1 | 1 |
| D4 | 0 | 1 | 0 | 0 |
| D5 | 0 | 1 | 0 | 1 |
| D6 | 0 | 1 | 1 | 0 |
| D7 | 0 | 1 | 1 | 1 |
| D8 | 1 | 0 | 0 | 0 |
| D9 | 1 | 0 | 0 | 1 |

# Priority encoder:

A priority encoder is a circuit or algorithm that compresses multiple binary inputs into a smaller number of outputs. The output of a priority encoder is the binary representation of the original number starting from zero of the most significant input bit. They are often used to control interrupt requests by acting on the highest priority request. If two or more inputs are given at the same time, the input having the highest priority will take precedence.

In this experiment a 4-to 2 priority encoder with a priority sequence of 2,1,3,0 has been shown. It means, in this priority encoder 2 has the highest priority and 0 has the lowest. If 2 is high then other numbers are ignored (even if any of them are high at the same time) and output would be binary representation of 2, i.e., Y1Y0=10. If 2 is found to be low, then next priority is given to 1. So, in this case if 1 is high, then 3 and 0 are ignored and output will be binary representation of 1, i.e., Y1Y0=01 and so on.

A diagram of a circuit

Description automatically generated

**Fig .3:** 4-to 2 priority encoder with a priority sequence of 2,1,3,0

The expressions for implementing the above priority encoder–

Y0 = A2’.A1 + A3.A2’.A1’ Y1 Y1= A2 + A3.A2’.A1’

Truth table for this priority encoder is given below –

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| A3 | A2 | A1 | A0 | Y1 | Y0 |
| x | 1 | x | x | 1 | 0 |
| x | 0 | 1 | x | 0 | 1 |
| 1 | 0 | 0 | x | 1 | 1 |
| 0 | 0 | 0 | 1 | 0 | 0 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Apparatus:** | | | |
| NOT Gate - | IC 7404 | 1[pcs] |
| AND Gate - | IC 7408 | 1[pcs] |
| OR Gate - | 5 input OR | 1[pcs] |
|  | 4 input OR | 2[pcs] |
|  | 2 input OR | 1[pcs] |

# Simulation and Measurement:

Part II

A diagram of a circuit

Description automatically generated**2-to-4 line decoder**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| A | B | D0 | D1 | D2 | D3 |
| 0 | 0 | 1 | 0 | 0 | 0 |
| 0 | 1 | 0 | 1 | 0 | 0 |
| 1 | 0 | 0 | 0 | 1 | 0 |
| 1 | 1 | 0 | 0 | 0 | 1 |

Truth table for 2-to-4 line decoder is given below –

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=0; B=0; =1; *; ;* | **A circuit board with wires and switches  Description automatically generated** |
| A=0; B=0; =0; *; ;* |  |
| A=0; B=0; =0; *; ;* |  |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=0; B=0; =0; *; ;* |  |

**Decimal to BCD encoder**

Truth table for decimal to BCD encoder is given below –

**A diagram of a number of numbers

Description automatically generated**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Dec. | Y3 | Y2 | Y1 | Y0 |
| D0 | 0 | 0 | 0 | 0 |
| D1 | 0 | 0 | 0 | 1 |
| D2 | 0 | 0 | 1 | 0 |
| D3 | 0 | 0 | 1 | 1 |
| D4 | 0 | 1 | 0 | 0 |
| D5 | 0 | 1 | 0 | 1 |
| D6 | 0 | 1 | 1 | 0 |
| D7 | 0 | 1 | 1 | 1 |
| D8 | 1 | 0 | 0 | 0 |
| D9 | 1 | 0 | 0 | 1 |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| D1=0;D2=0;D3=0;D4=0;D5=0;D6=0;D7=0;D8=0;D9=0 Y0=0;Y1=0;Y2=0;Y3=0 |  |


|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| D1=1;D2=0;D3=0;D4=0;D5=0;D6=0;D7=0;D8=0;D9=0 Y0=1;Y1=0;Y2=0;Y3=0 |  |
| D1=0;D2=1;D3=0;D4=0;D5=0;D6=0;D7=0;D8=0;D9=0 Y0=0;Y1=1;Y2=0;Y3=0 |  |
| D1=0;D2=0;D3=1;D4=0;D5=0;D6=0;D7=0;D8=0;D9=0 Y0=1;Y1=1;Y2=0;Y3=0 |  |
| D1=0;D2=0;D3=0;D4=1;D5=0;D6=0;D7=0;D8=0;D9=0 Y0=0;Y1=0;Y2=1;Y3=0 |  |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| D1=0;D2=0;D3=0;D4=0;D5=1;D6=0;D7=0;D8=0;D9=0 Y0=1;Y1=0;Y2=0;Y3=0 |  |
| D1=0;D2=0;D3=0;D4=0;D5=0;D6=1;D7=0;D8=0;D9=0 Y0=0;Y1=0;Y2=1;Y3=0 |  |
| D1=0;D2=0;D3=0;D4=0;D5=0;D6=0;D7=1;D8=0;D9=0 Y0=1;Y1=1;Y2=1;Y3=0 |  |
| D1=0;D2=0;D3=0;D4=0;D5=0;D6=0;D7=0;D8=1;D9=0 Y0=0Y1=0;Y2=0;Y3=1 |  |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| D1=0;D2=0;D3=0;D4=0;D5=0;D6=0;D7=0;D8=0;D9=1 Y0=1;Y1=0;Y2=0;Y3=1 |  |

**4-to 2 priority encoders with a priority sequence of 2,1,3,0**

Truth table for this priority encoder is given below.



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| A3 | A2 | A1 | A0 | Y1 | Y0 |
| x | 1 | x | x | 1 | 0 |
| x | 0 | 1 | x | 0 | 1 |
| 1 | 0 | 0 | x | 1 | 1 |
| 0 | 0 | 0 | 1 | 0 | 0 |

|  |  |
| --- | --- |
| SIMULATION | SIMULATION |
| **A computer screen shot of a diagram  Description automatically generated** | **A computer screen shot of a diagram  Description automatically generated** |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| **A computer screen shot of a diagram  Description automatically generated** | **A computer screen shot of a diagram  Description automatically generated** |

**Discussion**

The main purpose of this experiment is to understand the functionality of MUX, DEMUX, Encode and decoder circuits. A multiplexer (or mux) is a device that selects one of several inputs and forwards the selected input into a single line. A multiplexer of 2n inputs has n selection lines, which are used to select which input must be sent to the output. A multiplexer is also called a data selector. A demultiplexer (or demux) is a device taking a single input and selecting one of many data-output-lines, which is connected to the single input. An encoder is a device or a circuit that converts information from one format or code to another. A decoder does the reverse operation of the encoder. It undoes the encoding so that the original information can be retrieved. Both the encoder and decoder are combinational circuits. So throughout the experiment, we simulated the circuits of these circuits in multisim software and verified it with the truth table. Then we implemented the circuit in trainer board. While implementing the hardware oart, there were some difficulties we faced like loose connection, problem in the output led, and problem in the input switches. We investigated these issues and solved them.

# Reference:

<http://www.tutorialspoint.com/computer_logical_organization/combinational_circuits.htm>

**Part I**

**4to1 Multiplexer**


## Table:1

|  |  |  |
| --- | --- | --- |
| S1 | S0 | f |
| 0 | 0 | D0 |
| 0 | 1 | D1 |
| 1 | 0 | D2 |
| 1 | 1 | D3 |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=0; B=0; =1; *; ;* |  |
| A=0; B=1; =0; *; ;* |  |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=1; B=0; =1; *; ;* |  |
| SIMULATION | HARDWARE |
| A=1; B=0; =0; *; ;* |  |

**Demultiplexer**



**1 to 4 Demultiplexer**

## Table:2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S1 | S0 | D0 | D1 | D2 | D3 |
| 0 | 0 | Din | 0 | 0 | 0 |
| 0 | 1 | 0 | Din | 0 | 0 |
| 1 | 0 | 0 | 0 | Din | 0 |
| 1 | 1 | 0 | 0 | 0 | Din |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=0; B=0; =1; *; ;* | **A circuit board with wires and switches  Description automatically generated** |

|  |  |
| --- | --- |
| SIMULATION | HARDWARE |
| A=0; B=1; =1; *; ;* **A computer screen shot of a diagram  Description automatically generated** | **A circuit board with wires and switches  Description automatically generated** |

|  |  |
| --- | --- |
| **A computer screen shot of a diagram  Description automatically generated**A=1; B=0; =0; *; ;* | **A white electronic device with many wires  Description automatically generated** |
| A=1; B=1; =0; *; ;* |  |